HEIGHTS > 2.0m – LADDER

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 16 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** Pole strap or harness system, safety footwear appropriate to task  |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | General | All persons instructed in use of ladder | Supervisor |
| Daily periodical monitoring for compliance with WH&S Regulation | Supervisor |
| Fall | Ladder marked with load rating of at least 120kg and industrial type | User |
| Extension ladder not to exceed 7.5m except for use in a confined space | User |
| Ladder angle between 70° & 80° or 1:4 except for use in a confined space | User |
| Ladder placed on stable surface | User |
| Ladder securely anchored top & bottom | User |
| Three point contact maintained at all times | User |
| Use of a ladder strap or fall arrest harness system | User |
| Loss of foot hold | Safety footwear appropriate to the task | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7