HEIGHTS > 2.0m – HARNESS, TRIPOD & HAND WINCH

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 15 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Harness, spreader bar, safety footwear appropriate to task | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of tripod/davit, winch & harness | | Supervisor | |
| Daily periodical monitoring for compliance with WH&S Regulation | | Supervisor | |
| Fall | | Hand winch fitted to tripod/davit | | Supervisor | |
| Tripod/davit secured in position | | Supervisor | |
| Winch operator in place | | Supervisor | |
| Harness fitted to persons correctly (use buddy system) | | User | |
| Spreader bar used if required | | User | |
| Winch line connected to harness or spreader bar as required | | User | |
| User remains connected to winch line | | User | |
| Loss of foot hold | | Safety footwear appropriate to the task | | User | |
| Injury after fall | | No protruding items below | | User | |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7